Pixie Virtual Machine Video Layout

**0xA000 – 0xAFFF** – Video ram, points to character generator ROM

**0xB000 – 0xBFFF** – Color RAM, 50 rows x 80 columns of characters. 256 possible color values

**0xC000 – 0xC7FF** – Character generator ROM (2,048 bytes) – Code Page 437 format, 256 characters, 8 bytes-per characters, 8 rows of 8 pixels each.